RME Intelligent Audio Solutions

Digiface AVB / Dante

Network Driver Package for Windows 8/10/11

Includes driver for internal USB Ethernet adapter and AVB Controller

Important Information on network driver version 0.9908 and AVB Controller 09908.107


Installation
-------------

Follow the instructions of the RME Driver Install Wizard. With the Digiface Dante the AVB Controller can be deselected as it is only needed for the Digiface AVB.

-------------------------


News, changes and fixes

V 0.9908_09908.108 (11/11/2025)

- Fix buffer overrun while converting UTF8 to Unicode

-------------------------------

V 0.9908_09908.107 (10/07/2025)

- Fix memory error in AVB endpoint

- Dynamic mappings only for input streams

- Mappings no longer Show up multiple times

- Requesting Milan version, compatibility level Milan 1.2.

-------------------------------

V 0.9908_09908.108 (11/11/2025)

- Fix memory error in AVB endpoint

- Dynamic mappings only for input streams

- Mappings no longer Show up multiple times

- Requesting Milan version, compatibility level Milan 1.2.


-------------------------------

V 0.9907_09907.104 (07/07/2025)

- Improved memory access

-------------------------------

V 0.9891_09891.104 (06/25/2025)

- Fix installer: Selecting Digiface Dante also installed parts of the AVB Controller

New in AVB Controller 09891.104:

- Added scrollbars in the following dialogs: Stream Connections, Presentation Time Offset, Stream Formats

- Bug fix for large dialog windows: alignment of elements corrected

- Scaling of dialogs follows font size

-------------------------


V 0.9891_09891.101 (06/20/2025)

- Text edits in the installer's GUI

New in AVB Controller 09891.101:

- Fix for possible crash when scrolling in list boxes

-------------------------

V 0.9891_09891.100 (06/16/2025)

New in AVB Controller 09891.100

- Improved Milan compatibility: Static vs. dynamic mappings: Inputs use dynamich mappings, outputs use static mappings. Recognizes different Milan MVUs.


-------------------------


V 0.9891 (04/28/2025)

New in AVB Controller 0.9891

- Support for the new Class Compliant network mode of Digiface Dante (firmware v61 and up) and Digiface AVB (firmware v265 and upr)

- Improved support of Milan sample rate switching

- Minimum window size is set after restart when window is smaller than that

- Closing a dialog with X did not work


-------------------------


New in AVB Controller 0.9880

- Change from NDIS 6.0 to NDIS 6.3


-------------------------
 

New in AVB Controller 0.9847

- Digiface AVB now upports Milan compatible sample rate switching


-------------------------


New in AVB Controller 0.9846

- AVB Controller now supports High DPI

- Evaluation of the Available Index when establishing a connection (for example when unplugging/plugging the network cable) 

- HDSPe AoX card: extended dialog elements and new sync display

- Reduced bandwidth for AAF streams 


--------------------------------



Copyright RME 11/2025
All rights reserved. Windows 7/8/10/11 are trademarks of Microsoft Corporation. ASIO is a trademark of Steinberg Media Technologies GmbH.

